FIDDES PINE WATER BASED STAIN
PREPARATION	
Sand the wooden substrate in stages, working with a medium sandpaper (120 grit), through to a medium / fine grade (180 – 220 grit). Always sand in the direction of the grain pattern where possible, ensuring the removal of any blemishes and glue residue prior to the application of Fiddes Wood Dyes. Take care to remove all traces of sanding dust and test the chosen Fiddes Wood Dye on a similar substrate to verify colour / shade.
Stir the contents well and always check the shade before application.
APPLICATION	
Take a clean, lint free cotton cloth or sponge and apply in the direction of the wood grain where possible. Take care to remove any excess stain immediately with a separate, clean absorbent cloth, again following the direction of the grain pattern. To obtain a uniform colour, always wipe evenly, blending the stain over the whole surface area by exerting a degree of pressure when applying by hand. Leave to dry, and do not sand between coats.
The application of additional coats will deepen the existing colour / shade.
DRY TIME	
1 hour at room temperature.
COVERAGE	
16 sqm per Litre (depending on substrate and method of application)
COATS	
1 coat – further coats will deepen colour / shade.
THINNERS	
Water
RECOMMENDED FOR USE ON	
Fine Furniture, Doors, Floors, Cabinet Work and Panelling.
PACKAGING	
1lt, 2lt, 5lt, 25lt, containers.